**FOCA-UAS-PDRA-G02-APP Issue 1 Revision 0**

Application to PDRA – G01 Version 1.1 (AMC3 to Article 11 IR (EU) 2019/947)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **General Information** | | | | | |
| 0.1 | UAS Operator Data | | | | |
| 0.11 | UAS Operator Identification (ID) | | Enter text… | | |
| 0.12 | UAS Operator Name | | Enter text… | | |
| 0.13 | Accountable Manager (if applicable) | | Enter text… | | |
| 0.14 | Operational point of contact | | Name: Enter text…  Address: Enter text…  Phone: Enter text…  E-Mail: Enter text… | | |
| 0.2 | UAS Manufacturer / Type Certificate holder | | Enter text… | | |
| 0.3 | UAS Model name | | Enter text… | | |
| 0.4 | Type of UAS configuration | | Conventional Airplane  Helicopter  Multirotor | | Hybrid/VTOL  Lighter than air  Other, please specify: Enter text… |
| 0.5 | Do you tether the UAV during the operation? | | Yes  No | | |
| 0.6 | Maximum characteristic dimension [m] | | Enter text… | | |
| 0.7 | Maximum take-off mass [kg] | | Enter text… | | |
| 0.8 | UAS speeds [m/s] | | Fixed-wing: Cruise speed = Enter text…  Rotorcraft: Maximum speed = Enter text…  [optional]  Max rate of climb = Enter text…  Max rate of descent = Enter text… | | |
| 0.9 | Is there a [DVR](https://www.easa.europa.eu/newsroom-and-events/press-releases/easa-issues-guidelines-design-verification-drones-operated) or a [TC](https://www.easa.europa.eu/domains/aircraft-products/aircraft-certification) for this operation and UAS? | | Yes  No  If ‘yes’, please specify: Enter text… | | |
| 0.10 | Number of UAS and serial number(s) | | Enter text… | | |
| 0.11 | Description of proposed operations including the locations | | Please provide the GPS coordinates for the operational volume (flight geography and contingency volume), the ground risk buffer and the air risk buffer (if available) as a separate file using either .txt; .kmz or .kml.  Give reference to the file and section:  Enter text… | | |
| Short description of proposed operations  Enter text… | | | | |
| **Declaration of compliance** | | | | | |
| I, the undersigned, hereby declare that the UAS operation will comply with:   * any applicable European Union and national regulations * the applicable requirements of Regulation (EU) 2019/947; and * the limitations and conditions defined in the operational authorisation provided by the competent authority.   Moreover, I declare that the related insurance coverage, if applicable, will be in place at the start date of the UAS operation. | | | | | |
| **Place and Date**  Specify Location…  Specify date… | | **Name and Signature** | | ***FOR FOCA ONLY*** | |

**Compliance Matrix for PDRA – G02 Version 1.1**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | **PDRA characterisation and conditions** | |  |
| **Topic** | **Method of Assurance** | **Condition** | **Demonstration of Integrity** | **Demonstration of Assurance** |
|  |  | 1. **Operational characterisation (scope and limitations)** | |  |
| **Level of human intervention** | Self-declaration | 1.1 No autonomous operations: the remote pilot should have the ability to maintain control of the UA, except in case of a loss of the command-and-control (C2) link. | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 1.2 The remote pilot should operate only one UA at a time. | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 1.3 The remote pilot should not operate the UA from a moving vehicle. | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 1.4 The remote pilot should not hand the control of the UA over to another command unit. | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| **UA range limit** | Self-declaration | 1.5 Launch/recovery: At VLOS distance from the remote pilot, if not operating from a safe prepared area.  *Note: ‘safe prepared area’ means a controlled ground area that is suitable for the safe launch/recovery of the UA.* | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 1.6 In flight: The range limit should be within the coverage of the direct C2 link coverage (radio line of sight), which ensures the safe conduct of the flight. | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text…  *OR*  ”n/a” | ”I declare compliance.”  *OR*  ”n/a” |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Overflown areas** | Declaration supported by data | 1.7 UAS operations should be conducted over sparsely populated areas. | | | | Please describe how the population density data is identified.  Please include a reference to the relevant chapter/section of the OM where the procedures for determining the population density are provided.  Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | | ”I declare compliance.” |
| **UA limitations** | Self-declaration | 1.8 Maximum characteristic dimension (e.g.  wingspan, rotor diameter/area or maximum distance between rotors in case of a multirotor):  3 m | | | | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | | ”I declare compliance.” |
| 1.9 Typical kinetic energy (as defined in paragraph  2.3.1(k) of AMC1 to Article 11 of the UAS  Regulation: up to 34 kJ | | | | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | | ”I declare compliance.” |
| **Flight height limit** | Self-declaration | 1.10 The maximum height of the operation volume is limited by the size of the reserved or segregated airspace.  *Note: In addition to the vertical limit of the operational volume, an air risk buffer is to be considered (see ‘Air risk’ under point 3 of this table).* | | | | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | | ”I declare compliance.” |
| **Airspace** | Self-declaration | 1.11 Operations should only be conducted in airspace that is reserved or segregated for the purpose of conducting UAS operations (corresponding to an air risk that can be classified as ARC-a). | | | | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | | ”I declare compliance.” |
| **Visibility** | Self-declaration | 1.12 If take-off and landing are conducted in VLOS of the remote pilot, the visibility should be sufficient to ensure that no people are in danger during the take-off/landing phase. The remote pilot should abort the take-off or landing in case people on the ground are in danger. | | | | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text…  *OR*  ”n/a” | | ”I declare compliance.”  *OR*  ”n/a” |
| **Others** | Self-declaration | 1.13 The UA should not be used to drop material or to carry dangerous goods, except for dropping items in connection with agricultural, horticultural or forestry activities where the carriage of such items does not contravene any other applicable regulations. | | | | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | | ”I declare compliance.” |
| 1. **Operational risk classification (according to the classification defined in AMC1 to Article 11 of the UAS Regulation)** | | | | | | | | |
| **Final GRC** | 3 | | **Final ARC** | ARC-a | **SAIL** | | II | |
| 1. **Operational mitigations** | | | | | | | | |
| **Operational volume (see Figure 2 of AMC1 Article 11)** | Self-declaration | 3.1 To determine the operational volume, the UAS operator should consider the position-keeping capabilities of the UAS in 4D space (latitude, longitude, height, and time). | | | | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | | ”I declare compliance.” |
| 3.2 In particular, the accuracy of the navigation solution, the flight technical error of the UAS, as well as the flight path definition error (e.g. map error) and latencies should be considered and addressed when determining the operational volume. | | | | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | | ”I declare compliance.” |
| 3.3 The remote pilot should apply the emergency procedures as soon as there is an indication that the UA may exceed the limits of the operational volume. | | | | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | | ”I declare compliance.” |
| **Ground risk** | Self-declaration | 3.4 The UAS operator should establish a ground risk buffer to protect third parties on the ground outside the operational volume. | | | | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | | ”I declare compliance.” |
| 3.4.1 The minimum criterion should be the use of the ‘1:1 rule’ (e.g. if the UA is planned to operate at a height of 150 m, the ground risk buffer should at least be 150 m). | | | | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | | ”I declare compliance.” |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | 3.5 The operational volume and the ground risk buffer should be all contained in a sparsely populated area. | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 3.6 The applicant should evaluate the area of operations typically by means of an on-site inspection or appraisal, and should be able to justify reduced density of people at risk in the operational area and the ground risk buffer. | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| **Air risk** | Self-declaration | 3.7 The operational volume, including the air risk buffer, if applicable, should be entirely contained in the reserved or segregated airspace. | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| **Observers** |  | n/a |  |  |
| 1. **UAS operator and UAS operations conditions** | | | | |
| **UAS operator and UAS operations** | Declaration supported by data | 4.1 The UAS operator should: |  |  |
| 4.1.1 develop an operations manual (OM) (for the template, refer to AMC1 UAS.SPEC.030(3)(e) and to the complementary information in GM1  UAS.SPEC.030(3)(e)); | Please describe how this condition is met.  Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance and that supporting evidence is included in the OM.” |
| 4.1.2 develop procedures to ensure that the security requirements applicable to the area of operations are complied during the intended operation; | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance and that supporting evidence is included in the OM.” |
| 4.1.3 develop measures to protect the UAS against unlawful interference and unauthorised access; | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance and that supporting evidence is included in the OM.” |
|  |  | 4.1.4 develop procedures to ensure that all operations comply with Regulation (EU) 2016/679 on the protection of natural persons with regard to the processing of personal data and on the free movement of such data; in particular, the UAS operator should carry out a data protection impact assessment, when this is required by the data protection national authority of the Member State with regard to the application of Article 35 of that Regulation; | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance and that supporting evidence is included in the OM.” |
| 4.1.5 develop guidelines for its remote pilots to plan UAS operations in a manner that minimises nuisance, including noise and other emissions-related nuisance, to people and animals; | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance and that supporting evidence is included in the OM.” |
| 4.1.6 develop an emergency response plan (ERP) in accordance with the conditions for a ‘medium’ level of robustness (please refer to AMC3 UAS.SPEC.030(3)(e); | Please describe how this condition is met.  Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance and that the ERP is available to the competent authority for review.” |
| 4.1.7 validate the operational procedures in  accordance with the conditions for a ‘medium’ level of robustness, which are included in AMC2 UAS.SPEC.030(3)(e); | Please describe how this condition is met.  Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance and that the ERP is available to the competent authority for review.” |
| 4.1.8 ensure the adequacy of the contingency and emergency procedures and prove it through any of the following:   1. dedicated flight tests; or 2. simulations, provided that the representativeness of the simulation means is proven for the intended purpose with positive results; or 3. any other means acceptable to the competent authority; and | Please describe how this condition is met.  Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance and that the description for meeting this condition is available to the competent authority for review.” |
|  |  | 4.1.9 have a policy that defines how the remote pilot and any other personnel in charge of duties essential to the UAS operation can declare themselves fit to operate before conducting any operation. | Please describe how this condition is met.  Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance and that the description for meeting this condition is available to the competent authority for review.” |
| 4.1.10 designate for each flight a remote pilot with adequate competency and other personnel in charge of duties essential to the UAS operation if needed; | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance and that supporting evidence is included in the OM.” |
| 4.1.11 ensure that the UAS operation effectively uses and supports the efficient use of the radio spectrum in order to avoid harmful interference; | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance and that supporting evidence is included in the OM.” |
| 4.1.12 keep for a minimum of 3 years and maintain up to date a record of the information on UAS operations, including any unusual technical or operational occurrences and other data as required by the declaration or by the operational authorisation; | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance and that recordkeeping data is available to the competent authority.” |
| 4.1.13 As part of the procedures contained in the OM (point 4.1.1 above), include the description of the following: |  |  |
| 1. The method and means of communication with the authority or entity responsible for the management of the airspace during the entire period of the reserved or segregated airspace being active, as mandated by the authorisation.   *Note: The communication method should be published in the NOTAM activating the reserved airspace to also allow coordination with manned aircraft.* | Please describe how this condition is met.  Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance and that evidence is available to the competent authority for review.” |
|  |  | 1. The member(s) of personnel in charge of duties essential to the UAS operation, who are responsible for establishing that communication. | Please describe how this condition is met.  Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance and that evidence is available to the competent authority for review.” |
| **UAS maintenance** | Self-declaration | 4.2 The UAS operator should: |  |  |
| 4.2.1 ensure that the UAS maintenance instructions that are defined by the UAS operator are included in the OM and cover at least the UAS manufacturer’s instructions and requirements when applicable; and | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 4.2.2 ensure that the maintenance staff follow the UAS maintenance instructions when performing maintenance. | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 4.2.3 keep for a minimum of 3 years and maintain up to date a record of the maintenance activities conducted on the UAS; | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 4.2.4 establish and keep up to date a list of the maintenance staff employed by the operator to carry out maintenance activities; | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 4.2.5 comply with point UAS.SPEC.100, if the UAS uses certified equipment. | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text…  *OR*  ”n/a” | ”I declare compliance.”  *OR*  ”n/a” |
| **External services** | Self-declaration | 4.3 The UAS operator should ensure that the level of performance for any externally provided service that is necessary for the safety of the flight is adequate for the intended operation. The UAS operator should declare that this level of performance is adequately achieved. | Please describe how this condition is met.  Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | 4.4 The UAS operator should define and allocate the roles and responsibilities between the UAS operator and the external service provider(s), if applicable. | Please describe how this condition is met.  Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 1. **Conditions for the personnel in charge of duties essential to the UAS operation** | | | | |
| **General** | Self-declaration | 5.1 The UAS operator should ensure that all  personnel in charge of duties essential to  the UAS operation are provided with  competency-based theoretical and  practical training specific to their duties,  which consists of the applicable  theoretical elements derived from  AMC1 UAS.SPEC.050(1)(d) and practical  elements from AMC2 UAS.SPEC.050(1)(d)  and UAS.SPEC.050(1)(e). | Please describe how this condition is met.  Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.  Evidence of training are available for inspection at the request of the competent authority or its authorised representative. The training programme is documented in Enter text…”. |
| 5.2 The UAS operator should keep and  maintain up to date a record of all the  relevant qualifications and training  courses completed by the remote pilot and the other personnel in charge of  duties essential to the UAS operation and  by the maintenance staff for at least  3 years after those persons have ceased  to be employed by the organisation or  have changed position within the  organisation. | Please describe how this condition is met.  Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.”  Record-keeping data is available for inspection at the request of the competent authority. |
| **Remote pilot** | Self-declaration | 5.3 The remote pilot should have the  authority to cancel or delay any or all  flight operations under the following  conditions: | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 5.3.1 when the safety of persons is jeopardised; or | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 5.3.2 when property on the ground is jeopardised; or | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | 5.3.3 when other airspace users are jeopardised; or | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 5.3.4 when there is a violation of the terms of the operational authorisation | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
|  | 5.4 The remote pilot should: |  |  |
| 5.4.1 not perform duties under the influence of psychoactive substances or alcohol, or when they are unfit to perform their tasks due to injury, fatigue, medication, sickness or other causes; | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 5.4.2 be familiar with the manufacturer’s instructions provided by the manufacturer of the UAS; | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 5.4.3 ensure that the UA remains clear of clouds; | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 5.4.4 perform unaided visual scan of the airspace, as required, to avoid any potential collision hazard; | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 5.4.5 obtain updated information relevant to the intended operation about any  geographical zones defined in accordance with Article 15; and | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 5.4.6 ensure that the UAS is in a safe condition to  complete the intended flight safely and, if applicable, check whether the direct remote identification is active and up to date. | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| **Multi-crew coordination**  **(MCC)** | Self-declaration | 5.5 Where multi-crew coordination (MCC) may be required, the UAS operator should: |  |  |
| 5.5.1 designate a remote pilot-in-command to be responsible for each flight; | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text…  *OR*  ”n/a” | ”I declare compliance.”  *OR*  ”n/a” |
| 5.5.2 include procedures to ensure coordination between the remote crew members through robust and effective communication channels; those procedures should cover, as a minimum: | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text…  *OR*  ”n/a” | ”I declare compliance.” *OR*  ”n/a” |
|  |  | 5.5.2.1 the assignment of tasks to the remote crew members; and | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text…  *OR*  ”n/a” | ”I declare compliance.” *OR*  ”n/a” |
| 5.5.2.2 the establishment of step-by-step communication; and | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text…  *OR*  ”n/a” | ”I declare compliance.”  *OR*  ”n/a” |
| 5.6 ensure that the training of the remote crew covers MCC. | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text…  *OR*  ”n/a” | ”I declare compliance.”  *OR*  ”n/a” |
| **Maintenance**  **staff** | Declaration supported by data | 5.7 Any staff member that is authorised by the UAS operator to perform maintenance activities should have been adequately trained in the documented maintenance procedures. | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance and that supporting evidence is included in the OM.”  Evidence of training is available at the request of the competent authority. |
| **Personnel in charge of duties essential to the UAS operation are fit to operate** |  | 5.8 The personnel in charge of duties essential to the UAS operation should declare that they are fit to operate before conducting any operation, based on the policy that is defined by the UAS operator | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 1. **Technical conditions** | | | | |
| **General** | Self-declaration | 6.1 The UAS should be equipped with means to monitor the critical parameters of a safe flight, in particular the following: |  |  |
| 6.1.1 the UA position, height or altitude, ground speed or airspeed, attitude, and trajectory; | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 6.1.2 the UAS energy status (fuel, battery charge, etc.); and | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 6.1.3 the status of critical functions and systems; as a minimum, for services based on RF signals (e.g. C2 link, GNSS, etc.), means should be provided to monitor the adequate performance and trigger an alert when the performance level becomes too low. | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| **Human-machine interface (HMI)** | Self-declaration | 6.2 The UAS information and control interfaces should be clearly and succinctly presented and should not confuse, cause unreasonable fatigue, or contribute to causing any disturbance to the personnel in charge of duties essential to the UAS operation in such a way that could adversely affect the safety of the operation. | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | 6.3 The UAS operator should conduct a UAS evaluation that considers and addresses human factors to determine whether the HMI is appropriate for the operation. | Please describe how this condition is met.  Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| **C2 links and communication** | Self-declaration | 6.4 The UAS should comply with the applicable requirements for radio equipment and the use of the RF spectrum. | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 6.5 Protection mechanisms against interference should be used, especially if unlicensed bands (e.g. ISM) are used for the C2 link (mechanisms such as FHSS, DSSS or OFDM technologies, or frequency deconfliction by procedure). | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 6.6 The UAS should be equipped with a C2 link that is protected against unauthorised access to the command-and-control functions. | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 6.7 In case of loss of the C2 link, the UAS should have a reliable and predictable method to recover the command-and-control link of the UA or to terminate the flight in a way that reduces any undesirable effect on third parties in the air or on the ground. | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 6.8 The UAS operator should ensure that reliable and continuous means of two-way communication for the purpose that is indicated in point 4.13(a) above are available. | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| **Tactical mitigation** |  | n/a | | |
| **Containment** | Declaration supported by data | 6.9 To ensure a safe recovery from a technical issue that involves the UAS or an external system that supports the operation, the UAS operator should ensure that: |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | 6.9.1 no probable failure of the UAS or of any external system that supports the operation would lead to operation outside the operational volume; and | Please describe how this condition is met.  Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.”  A design and installation appraisal is available and it covers at least:   * the design and installation features (independence, separation, and redundancy); and * the particular risks (e.g. hail, ice, snow, electromagnetic interference, etc.) relevant to the type of operation. |
| 6.9.2 it is reasonably expected that a fatality will not occur due to any probable failure of the UAS or of any external system that supports the operation.  *Note: The term ‘probable’ should be understood in its qualitative interpretation, i.e. ‘anticipated to occur*  *one or more times during the entire system/operational life of an item’.* | Please describe how this condition is met.  Document name: Enter text…  Chapter number: Enter text… |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Declaration supported by data | 6.10 The following additional conditions should apply if the adjacent area includes an assembly of people or if the adjacent airspace is classified as ARC-d (in accordance with the SORA). |  |  |
| 6.10.1 The UAS should be designed to standards that are considered adequate by the competent authority and/or in accordance with a means of compliance that is acceptable to that competent authority such that: | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text…  *OR*  ”n/a” | ”I declare compliance.”  Analysis and/or test data with supporting evidence is available. |
| * + - 1. the probability of the UA leaving the operational volume should be less than 10-4/FH; and | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text…  *OR*  ”n/a” |
| * + - 1. no single failure of the UAS or of any external system that supports the operation should lead to operation outside the ground risk buffer.   *Note: The term ‘failure’ should be understood as an occurrence that affects the operation of a component, part, or element in such a way that it can no longer function as intended. Errors may cause failures but are not considered to be failures. Some structural or mechanical failures may be excluded from the criterion if it can be shown that these mechanical parts were designed according to aviation industry best practices.* | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text…  *OR*  ”n/a” |  |
| 6.10.2 SW and AEH whose development error(s) could directly lead to operations outside the ground risk buffer should be developed according to an industry standard or methodology that is recognised as adequate by the competent authority.  *Note 1: The proposed additional safety conditions cover both the integrity and the assurance levels.*  *Note 2: The proposed additional safety conditions do not imply a systematic need to develop the SW and AEH according to an industry standard or methodology that is recognised as adequate by the competent authority. For instance, if the UA design includes an independent engine shutdown function that systematically prevents the UA from exiting the ground risk buffer due to single failures or an SW/AEH error of the flight controls from occurring, the intent of the conditions of point 6.10.1 above could be considered met* | Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text…  *OR*  ”n/a” |
| **Remote**  **identification[[1]](#footnote-1)** | Self-declaration | 6.11 The UAS has a unique serial number compliant with standard ANSI/CTA-2063-A-2019, *Small Unmanned Aerial Systems Serial Numbers*, 2019, according to Article 40(4) of Regulation (EU) 2019/945. | Please describe how this condition is met.  Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.” |
| 6.12 The UAS is equipped with a remote identification system according to Article 40(5) of Regulation (EU) 2019/945. | Please describe how this condition is met.  Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text… | ”I declare compliance.”.” |
| **Lights[[2]](#footnote-2)** | Self-declaration | 6.13 If the UAS is operated at night, it is equipped with at least one green flashing light according to  point UAS.SPEC.050(1)(l)(i) of the UAS Regulation. | Please describe how this condition is met.  Document name: Enter text…  Chapter number: Enter text…  Page number: Enter text…  *OR*  ”n/a” | ”I declare compliance.”  *OR*  ”n/a” |
|  |  |  | |  |
| **Contact E-Mail, Place, and Date** | |  | **Name and Signature** |  |

1. Applicable from 1 July 2022. [↑](#footnote-ref-1)
2. Applicable from 1 July 2022. [↑](#footnote-ref-2)